|  |
| --- |
| **Instructions Stadtkirche Wittenberg** |

**Base plate**

|  |  |
| --- | --- |
| **Page 1 (Seite 1)**  Cut out the hatched fields on part 1, to make the inside accessible, which helps the assembly.  **Main nave**  **Page 2 & 3 (Seite 2 & 3)**  Parts 2 and 3 are the outer walls of the main nave. Cut them out accurately, score, fold and glue to the base plate and to one another. | Ohne Titel-1.jpg |

|  |  |
| --- | --- |
| The buttresses 2a – 2e as well as 3b – 3c can be glued on the walls before or after the walls are glued to the base plate. They consist of a long inner part and a shorter outer part, which together form buttresses with squared section.  Keep save the small parts 11 and 12  Attach the entrance hall 3a to part 3. | Skizze-6.jpg |

**Towers**

|  |  |
| --- | --- |
| **Page 4 (Seite 4)**  Part 4 becomes the north tower, a squared pillar with top covered.  **Page 5 (Seite 5)**  Part 5 is a connecting building between the two towers, it has a roof part, which is 5a  Keep save part 9  **Page 6 (Seite 6)**  Part 6 becomes the south tower.  The south tower equals the north tower, only mirrored. The towers should not be mixed up. Both must be attached exactly on the base plate as well as on the white wall of part 3.  Parts 4a and 5a are railings. These are scored in the middle, then folded in and out and glued to become inner and outer side. Then corners are bluntly glued together.  Parts 6b – 6d are forming a bridge, which connects the two tower platforms. These parts have a railing as well, which is handled the same way. | **Skizze-5.jpg** |

**Nave extension  
Page 7**

First cut part 7a out of the white area of part 7

Parts 7 and 8 are the outer walls of the Nave extension and are constructed in the same way as parts 2 and 3.

The buttresses of this part of the building are very different from one another. Part 8f is has a triangular section. All other buttress parts have rectangular sections, same as on those attached to walls (parts) 2 and 3.

The glue tab on part 8d is glued with one half to 8e. Then that new part is turned around and glued to the backside of the protruding stepped section of the gable.  
8g is a wall altar. The right half is glued to part 8 and the left half is glued onto the buttress 8f

**Roofs**

Next, the roof – part 9 (page 5) – is scored in the middle and glued on top of the Nave extension  
 **Page 8**keep save part 16

Das Dach Teil 10 ist besonders schwierig, weil es sehr groß ist und viele Klebelaschen berücksichtigt werden müssen. Hier hilft das Loch in der Grundplatte, durch das man von innen gegenhalten kann.

The main roof – part 10 – is a bit tricky, as it is rather big and many glue tabs have to be taken care of. Fortunately, a hole in the base plate was created to be of big help here.

**Stair towers / Vestry**  
  
Parts 11 and 12 are stair towers and each consist of wall part and roof part each.   
Parts 13 are for the vestry. Part 13b is another buttress and the tiny part 13c is glued to the front of it.  
  
**Tower tops  
  
Page 9**

Part 14 (north tower) and part 15 (south tower) are the tower tops of both towers.  
The construction for both towers is the same.

Part 14a (15a) is glued together to become an octagonal pillar. This is first attached to the roof of the tower. As the windows are not the same to all directions, one has to follow the markings on the parts (W is for west). At the end, the top is closed up.

|  |  |
| --- | --- |
| Part 14b (15b) is shaped to a bell-like shape. It’s best to glue each of the 8 petals separately, glued bluntly to each other and wait out until it has dried. Part 14b is glued centered on the top of 14a. When all has dried good enough, the outer ring 14c (15c) may be glued around the bell-shaped roof.  Parts 14d and 14e are the topmost part of the tower. When they are completely dry, the top may be pushed in a bit to let the roof appear somewhat bell-shaped as well.  **14 (15)** The final part is 16, the upper part of buttress 16a. To assemble this roof, it is best to use a pencil for help. | Skizze-2.jpg |

|  |  |
| --- | --- |
| P1020147-n mit Zahlen.jpg | P1020160 mit Zahlen.jpg |

Happy work!

It could be prudent to make a duplicate of the pages before starting the work to have backup in case something goes wrong or a single part gets lost.