Instructions general

Stahl Allendorf

|  |  |
| --- | --- |
| **Order** of work steps in general:  1. score   2. Cut out  3. fold  4. glue  When scoring, it is necessary to work exactly, which means to score exactly along the drawn dashed lines. Since most score lines are straight, it is recommended to use a ruler. | falzen |

On some surfaces, the score lines are not seen as dashed but can only be seen across the edges of the part, which is cut off. In these cases, connect the two ends with a ruler and then score across the part.

Cutting should be done also as exact as possible along the ongoing lines. No white edges should remain.

The experienced modeler knows, where to cut bigger glue tabs. While bigger tabs require more glue, they also increase stability.

Generally the following holds true for assembly: First glue together the walls and attach to existing building parts, then put the roof on top.  
The glues PONAL or UHU are recommended. Usually, it helps to follow the numbers for the order of assembly.

**Lines and their meaning**

|  |  |
| --- | --- |
| Linien-3 | Cut out  Score & fold  Line, where another part is attached  Dashed lines with an X at the ends, must be scored from the backside and folded to the other side (valley fold). To help, the two x’s can be punctured with a needle, the holes of which can then be connected by scoring on the backside  This is an area that must be cut out. |

**To print out, 120-er paper** **(120 g/m2) is recommended**